Thanks for purchasing PLANET ICS-10X RS-232 / RS-422 / RS-485 over Fast Ethernet Media Converter.

This document provides the firmware release note and history of the product.

Version 1.7b Released at 2011/10/06

Firmware version: 1.7b110927
Hardware version: 1.0
Release at 2011/10/06 

Function enhance

This firmware provides the following modification:

A: Bug Fixed -

(1) Fix the catch CSS issue when clear cookie.

(2) Fix the Client reply signal loss

B. Function Added - 

(1) Change Inactive Timeout to be "Second"

 


Upgrade Requirements:

1. The latest firmware version of ICS-10X.
2. The ICS-10X RS-232 / RS-422 / RS-485 over Fast Ethernet Media Converter 
3. Workstation with Microsoft IE 7.0 or above.
4. TFTP server.


Upgrade procedure:

1. Connect the RJ-45 UTP cable to the target ICS-10X.
.
2. Login is required to access the WEB interface after the ICS-10X boot completes successfully. The factory default user name and password is "admin".

3. After Web main screen appeared, click the "System"\"Firmware Upgrade" at the left Menu.  

4. The screen will be direct to the "Firmware Upgrade" page, click "Load" button to erase old F/W in flash.

5. The "Firmware Upgrade Mode" displayed on the screen, click the "Browse" button of the main page, the system would pop-up the file selection menu to choose firmware.

6. Select on the firmware then click "Upgrade". The firmware upgrade may take 60 seconds. Please don't power off the ICS-10X while procedure be started.

7. Please wait until the successful message shows in the Update Status field.

8. Please wait until the system reboot complete.

9. Relogin the ICS-10X via WEB browser. Please click the "System" \ "System Information" to double check if the firmware be upgraded successfully.

 

*************************
Firmware Release History:  
*************************

===================================
Version 1.6b Released at 2010/10/22

Firmware version: 1.6b101022
Hardware version: 1.0
Release at 2010/10/22 
===================================

Function enhance

This firmware provides the following modification:

(1) Fix the change IP address issue.

(2) Fix the UDP client mode issue.

(3) Fix the software reset default that IP address can not become to default IP address.

B. Function Added - 

(1) N/A


===================================
Version 1.3b Released at 2009/01/14

Firmware version: 1.3b090114A
Hardware version: 1.0
Release at 2009/01/14 
===================================

Function enhance

This firmware provides the following modification:

A: Bug Fixed -

(1) Fix the error character issue.

(2) Enchance the serial interface transfer rate.

B. Function Added - 

(1) N/A

==================================
Version 1.2b Released at 2008/10/09

Firmware version: 1.2b081009A
Hardware version: 1.0
Release at 2008/10/09 
==================================

Function enhance

This firmware provides the following modification:

A: Bug Fixed -

(1) N/A

B. Function Added - 

(1) Add SMTP function - When "log-fail" and "operation mode" be changed, network manager will receive alert mail from ICS-10X.

(2) Support firmware upgrade under Firefox browser version 3.0.

===================================
Version 1.1a Released at 2008/06/11

Firmware version: 1.1a080611
Hardware version: 1.0
Release at 2008/06/11 
===================================
Initial release


Sincerely yours,
PLANET Technical Support Team
Http://www.planet.com.tw


