Thanks for purchasing PLANET WGSW-24040 / WGSW-24040R Switch.
This document provides the firmware release note and history of the product

Version 1.1b090901 Released at 2009/09/01
=============================
Firmware version: v1.1b090901
Hardware version: 1.x
File Name: FW-WGSW24040_v1.1b090901.dat
File Size: 2,269KB 
Release at 2009/09/01 
=============================
Function enhance

This firmware provides the following modification:

A: Bug Fixed -

   (1) Port-21~Port-24 fail to forward CPU ICMP Ping reply packets
   (2) Upgrade the eCOS kernel with higher version to solve the HTTP server unstable issue

B. Function Added -

   (1) [SNMP] SNMP RMON MIB support
   (2) [SNMP] SNMP Q-Bridge MIB support
   (3) [System] Display AC, DC power inpute status (WGSW-24040R only)
   (4) [System] Add temperature detection to display the inside operating temperature
   (5) 100FX SFP transceiver support

C. Other:
    (1) [SNTP] Modify the Time Display and Configure format in web page "SNTP Configuration"

D. Known Issue:
    (1) LACP + RSTP cause system halt
=============================================



[Upgrade Requirements]:

1. The latest firmware version of WGSW-24040 series
2. The WGSW-24040 / WGSW-24040R Switch
3. Workstation with Microsoft IE 6.0 or above.
4. TFTP server.


[Upgrade procedure]:

1. Connect the RJ-45 UTP cable to the target Switch.

2. Login is required to access the WEB interface after the Switch boot completes successfully. The factory default user name and password is "admin".

3. After Web main screen appeared, click the "System"\"TFTP Firmware Upgrade" at the left Menu.  

4. The screen will be direct to the "TFTP Firmware Upgrade" page, enter values as below.
   a. Enter TFTP IP address.
   b. Firmware File Name: please enter firmware file name, like as "FW-WGSW24040_v1.1b090901.dat"

5. Click "Upgrade" button to start the firmware upgrade procedure. 

6. The system would pop up the confirm message, Click ˇ§OKˇ¨, the Switch will start the TFTP upgrade procedure.

7. Please don't power off the Switch while procedure be started.

8. Please check your TFTP server application to confirm the TFTP file is well transmit to the Switch.

9. The Switch will reboot then, and It will cost 2 to 3 minutes for the TFTP firmware upgrade and reboot procedure. 
   Please wait for the process complete.

10. Once the new software is loaded to the system successfully, the Login screen appears. 

11. Enter the user name and password to login the Switch.

12. Relogin the Switch via WEB browser. Please click the "System \ "System Information" to double check if the firmware be upgraded successfully.

 

*************************
Firmware Release History:  
*************************


==================================
Version V1.0b080919
Released at 2008/09/19
==================================

Initial Release

Sincerely yours,
PLANET Technical Support Team
Http://www.planet.com.tw


