Thanks for purchasing PLANET HPOE-2400G(V2) Injector Hub Switch.
This document provides the firmware release note and history of the product

Version 2.0b Released at 2013/08/02

Firmware version: 2.0b130802
Release at 2013/08/10

This firmware provides the following modification:

Initial release

[Upgrade Requirements]:

1. The latest firmware version of HPOE-2400G(V2)
2. The HPOE-2400G(V2) Injector Hub Switch
3. Workstation with Microsoft IE 6.0 or above.


[Upgrade procedure]:

1. Connect the RJ-45 UTP cable to the target HPOE-2400G(V2) Injector Hub Switch.

2. Login is required to access the WEB interface after the switch boot completes successfully. The factory default user name and password is "admin".

3. After Web main screen appeared, click the "System --> Firmware Upgrade" at the left Menu.  

4. The screen provided HTTP Firmware Upgrade.

   A. HTTP Firmware Upgrade
     (1) Enter the "Browse.." button to locate firmware path.
     (2) Click "Submit" button to start the firmware upgrade procedure.Please don't power off the switch while procedure be started.
     (3) Please wait until the system reboot complete.
     (4) Reset to factory default again.

5. Relogin the switch via WEB browser. Please click the "System -->System Information --> Firmware Version" to double check if the firmware be upgraded successfully.



Sincerely yours,
PLANET Technical Support Team
Http://www.planet.com.tw


