PLANET GSD-1002M Firmware Release
==============================================
Product:GSD-1002M
Release Date:02/13/2015
Version:1.0b150211
File Size:5,617KB

Release Information:
=============
- Supports auto mode for SFP slots.
- Supports PLANET Smart Discovery Lite.
-	Bug fixed ¡V SNMP configuration could not be saved after reboot.
-	Bug fixed ¡V Removed dual image function.

Do not turn the power off during the upgrade process. This will damage the unit.

This firmware is for the GSD-1002M only, and please reset the device to the factory default setting after upgrading.
Please don't decompress firmware file (*.bix).
Before upgrading the GSD-1002M firmware, please disable your anti-Virus software first.
(because some anti-virus software will block the upgrade process)
And follow the steps below to upgrade GSD-1002M's firmware:
 Step 1. Logging in the GSD-1002M.
 Step 2. Go to the "Maintenance > Upgrade Manager" page.
 Step 3. Select "HTTP" in the drop-down menu.
 Step 4. Press the "Browse" button and select the correct firmware (*.bix) 
 Step 5. Press the "Upgrade" button to upgrade your GSD-1002M.
 Step 6. Press the "OK" button to reboot the GSD-1002M when the "Confirm" window pops out.
 Step 7. When the login screen appears, please press the hardware reset button for over 10 seconds to reset the GSD-1002M its default setting.

Support_switch@planet.com.tw
Update History
==========================
Firmware version: v1.0b140225
Hardware version: 1.0
==========================
Initial Release

