PLANET GSD-1020S Firmware Release
==============================================
Product: GSD-1020S
Release Date: 02/13/2015
Version: 1.0b150211
File Size: 5,616KB

Release Information:
=============
- Supports auto mode for SFP slots.
- Supports PLANET Smart Discovery Lite.
-	Bug fixed ¡V SNMP configuration could not be saved after reboot.
-	Bug fixed ¡V Removed dual image function.

Do not turn the power off during the upgrade process. This will damage the unit.

This firmware is for GSD-1020S only, and please reset the device to the factory default setting after upgrading.
Please don't decompress firmware file (*.bix).
Before upgrading the GSD-1020S firmware, please disable your anti-Virus software first.
(because some anti-virus software will block the upgrade process)
And follow the steps below to upgrade GSD-1020S's firmware:
 Step 1. Logging in the GSD-1020S.
 Step 2. Go to the "Maintenance > Upgrade Manger" page.
 Step 3. Select "HTTP" in the drop-down menu.
 Step 4. Click the "Browse" button and select the correct firmware(*.bix) 
 Step 5. Click the "Upgrade" button to upgrade your GSD-1020S.
 Step 6. Click the "OK" button to reboot the GSD-1020S when the "Confirm" window pops out.
 Step 7. When the login screen appears, please click the hardware reset button for over 10 seconds to reset the GSD-1020S its default setting.

Support_switch@planet.com.tw
Update History
==========================
Firmware version: v1.0b140225
Hardware version: 1.0
==========================
Initial Release

